# Blocksmith Hat-Block Stand Prototype 001

This is the matching stand used by the simplified V1 crown generator.

- Five BS-1.0 pegs at the center and ±40 mm cardinal offsets.
- Peg diameter: 24.606 mm.
- Working peg length: 23.813 mm.
- Intended crown sockets: Ø25.4 mm × 25.4 mm deep.
- Verified mesh: watertight by edge count, zero degenerate triangles.

Print the stand first. The optional fit-check in Blocksmith Studio can be used
when a printer/material combination needs troubleshooting.

This is a printable engineering prototype pending physical evaluation. It is
not certified for steam, heat, load-bearing, or production use.
